IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Time stamp: "2023-01-30T13:38:13"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190808_0900(x64) - Exporter 19.2.20.24 - Default UI"
Application: "Autodesk Revit 2019 (ENU)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENU)"

People and organizations
  Person "ryan.lashley24DJN" of Organization (no name given)
  Owner history of Person "ryan.lashley24DJN" of Organization (no name given) | application "Autodesk Revit 2019 (ENU)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENU)" | change NOCHANGE | created 1675085873 (2023-01-30T13:37:53Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCTRANSPORTELEMENT | type IFCTRANSPORTELEMENTTYPE "Height=0.15m(0'-6")_Reach=15.00m(49'-3")" | object type "Height=0.15m(0'-6")_Reach=15.00m(49'-3")" | ELEVATOR | names: "BoelsRental_18034_TelescopicBoomLift_JLG_1350SJP:Height=0.15m(0'-6")_Reach=15.00m(49'-3"):29295" | material: materials ("BoelsRental_Plastic_Blue", "BoelsRental_Plastic_Green", "BoelsRental_LightBlack", "BoelsRental_Plastic_Yellow", "JLG_Metal Paint_White", "JLG_Metal Paint_Black", "JLG_Paint_White", "JLG_Paint_Black", "BoelsRental_PrimaryMaterial", "JLG_Paint_Silver Grey", "JLG_Paint_Orange", "BoelsRental_LogoWhite", "BoelsRental_LogoBlack", "BoelsRental_Tire") | property sets: Pset_ManufacturerTypeInformation, Constraints, Construction, Dimensions, Other, Phasing

Types
  IFCTRANSPORTELEMENTTYPE "Height=0.15m(0'-6")_Reach=15.00m(49'-3")" | 1 occurrence | material: materials ("BoelsRental_Plastic_Blue", "BoelsRental_Plastic_Green", "BoelsRental_LightBlack", "BoelsRental_Plastic_Yellow", "JLG_Metal Paint_White", "JLG_Metal Paint_Black", "JLG_Paint_White", "JLG_Paint_Black", "BoelsRental_PrimaryMaterial", "JLG_Paint_Silver Grey", "JLG_Paint_Orange", "BoelsRental_LogoWhite", "BoelsRental_LogoBlack", "BoelsRental_Tire") | property sets: Constraints, Data, Identity Data, Model Properties, Other

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCTRANSPORTELEMENT)
    Manufacturer = "Boels Rental (JLG)" (IFCLABEL)
    ModelReference = "Telescopic Boom Lift" (IFCLABEL)
    ProductionYear = "2023" (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCTRANSPORTELEMENT)
    Host = "None" (IFCTEXT)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    P2 = FALSE (IFCBOOLEAN)
    P4 = FALSE (IFCBOOLEAN)
    PR = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Sa = 180. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    WE = 710. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 type object
    AE = 3851. (IFCLENGTHMEASURE) [MILLI METRE]
    AEa = -0.85 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    AEa1 = 179.15 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    E = 1283.66666666667 (IFCLENGTHMEASURE) [MILLI METRE]
    JHa = 0.85 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    JHa1 = 180.85 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Ja = -55.18 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Ja1 = 124.82 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    JibRotation = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    P230 = TRUE (IFCBOOLEAN)
    P450 = TRUE (IFCBOOLEAN)
    PHa = 55.18 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    PHa1 = 235.18 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reach = 4 (IFCINTEGER)
  Construction | properties | on 1 object (1 IFCTRANSPORTELEMENT)
    PlatformRotation = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    ReachDiagram = FALSE (IFCBOOLEAN)
    SwingAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    TurningRadiusExtended = FALSE (IFCBOOLEAN)
    TurningRadiusRetracted = FALSE (IFCBOOLEAN)
    WorkingArea = FALSE (IFCBOOLEAN)
  Dimensions | properties | on 1 object (1 IFCTRANSPORTELEMENT)
    Area = 2128.24185993277 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 11.2879346495038 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCTRANSPORTELEMENT)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "Please Record On Commissioning." (IFCTEXT)
    Category = "Site" (IFCLABEL)
    Family = "BoelsRental_18034_TelescopicBoomLift_JLG_1350SJP: Height=0.15m(0'-6")_Reach=15.00m(49'-3")" (IFCLABEL)
    Family and Type = "BoelsRental_18034_TelescopicBoomLift_JLG_1350SJP: Height=0.15m(0'-6")_Reach=15.00m(49'-3")" (IFCLABEL)
    InstallationDate = "Please Record On Commissioning." (IFCTEXT)
    SerialNumber = "Please Record On Commissioning." (IFCTEXT)
    Type = "BoelsRental_18034_TelescopicBoomLift_JLG_1350SJP: Height=0.15m(0'-6")_Reach=15.00m(49'-3")" (IFCLABEL)
    Type Id = "BoelsRental_18034_TelescopicBoomLift_JLG_1350SJP: Height=0.15m(0'-6")_Reach=15.00m(49'-3")" (IFCLABEL)
    WarrantyStartDate = "Please Record On Commissioning." (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Level 1" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level: Level 1" (IFCLABEL)
    Type Id = "Level: Level 1" (IFCLABEL)
  Other | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Movable" (IFCTEXT)
    Category = "Site" (IFCLABEL)
    ClassificationName = "Uniclass2015" (IFCTEXT)
    ClassificationValue = "TE_30_30_10_60" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    CreatedBy = "https://www.boels.com/" (IFCTEXT)
    CreatedOn = "2023-01-24T09:30:00" (IFCTEXT)
    DocumentationCertificates = "https://www.boels.com/" (IFCTEXT)
    DocumentationInstallationGuide = "https://www.boels.com/" (IFCTEXT)
    DocumentationLiterature = "https://www.boels.com/" (IFCTEXT)
    DocumentationMaintenance = "https://www.boels.com/" (IFCTEXT)
    DocumentationTechnical = "https://www.boels.com/" (IFCTEXT)
    DurationUnit = "Years" (IFCTEXT)
    ExpectedLife = 0 (IFCINTEGER)
    Family Name = "BoelsRental_18034_TelescopicBoomLift_JLG_1350SJP" (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Finish = "n/a" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    ManufacturerName = "Boels Rental (JLG)" (IFCTEXT)
    Material = "n/a" (IFCTEXT)
    ModelNumber = "Telescopic Boom Lift - 1350SJP" (IFCTEXT)
    ModelReference = "Telescopic Boom Lift" (IFCTEXT)
    ProductionYear = "2023" (IFCTEXT)
    ReferencedStandard = "n/a" (IFCTEXT)
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "n/a" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    TypeName = "Height=0.15m(0'-6") - Reach=15.00m(49'-3")" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "0" (IFCTEXT)
    WarrantyDurationParts = "0" (IFCTEXT)
    WarrantyDurationUnit = "Years" (IFCTEXT)
    WarrantyGuarantorLabor = "https://www.boels.com/" (IFCTEXT)
    WarrantyGuarantorParts = "https://www.boels.com/" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCTRANSPORTELEMENT)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "E1030100" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Cost = 0. (IFCREAL)
    Description = "Sturdy machine that makes you feel confident about working at a great height with a platform loading capacity of more than 450 kg." (IFCTEXT)
    Keynote = "X" (IFCTEXT)
    Manufacturer = "Boels Rental (JLG)" (IFCTEXT)
    Model = "Telescopic Boom Lift - 1350SJP" (IFCTEXT)
    OmniClass Number = "23.40.00.00" (IFCTEXT)
    OmniClass Title = "Equipment and Furnishings" (IFCTEXT)
    Type Comments = "Height=0.15m(0'-6") - Reach=15.00m(49'-3")" (IFCTEXT)
    Type Name = "Height=0.15m(0'-6")_Reach=15.00m(49'-3")" (IFCTEXT)
    URL = "https://www.boels.com/" (IFCTEXT)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Data | properties | on 1 type object
    ArticulatingJib = "2.44 m" (IFCTEXT)
    AuxiliaryPower = "12V DC" (IFCTEXT)
    AxleOscillation = "0.30 m (1 ft 0 in)" (IFCTEXT)
    BoelsProductName = "Telescopic boom lift, 43 m" (IFCTEXT)
    BoelsSubgroup = "18034" (IFCTEXT)
    DieselEngine = "Deutz BF4M2011 87HP (65.0 kw)" (IFCTEXT)
    DriveSpeed4WD = "5.2 km/h (3.25 mph)" (IFCTEXT)
    FuelTankCapacity = "117L(31 gal)" (IFCTEXT)
    Gradeability = "45%" (IFCTEXT)
    HorizontalOutreachRestricted = "21.34 m (70 ft 0 in)" (IFCTEXT)
    HorizontalOutreachUnrestricted = "24.38 m (80 ft 0 in)" (IFCTEXT)
    HydraulicPlatformRotator = "180 Degree" (IFCTEXT)
    HydraulicTankCapacity = "208 L (55 gal)" (IFCTEXT)
    JibOverallLength = "2.44m (8 ft 0 in)" (IFCTEXT)
    JibRangeOfArticulation = "130 Degrees (+75°/ 55°)" (IFCTEXT)
    MachineWeightANSI = "20,300kg (44,750 lbs)" (IFCTEXT)
    MachineWeightCE = "20,300kg (44,750 lbs)" (IFCTEXT)
    MaxGroundBearingPressureANSI = "7.38 kg/cm2 (105 psi)" (IFCTEXT)
    MaxGroundBearingPressureCE = "7.38 kg/cm2 (105 psi)" (IFCTEXT)
    NumberOfPeople = 0 (IFCINTEGER)
    PlatformCapacityRestrictedANSI = "450 Kg (1000 lbs)" (IFCTEXT)
    PlatformCapacityRestrictedCE = "450 Kg (1000 lbs)" (IFCTEXT)
    PlatformCapacityUnrestrictedANSI = "227 kg (500 lbs)" (IFCTEXT)
    PlatformCapacityUnrestrictedCE = "230 kg" (IFCTEXT)
    PlatformHeightRestricted = "38.35 m (125 ft 10 in)" (IFCTEXT)
    PlatformHeightUnrestricted = "41.30 m (135 ft 6 in)" (IFCTEXT)
    PlatformRotator = "180 degrees" (IFCTEXT)
    PlatformSideEntry = "0.91 m x 2.44 m (3 ft 0 in x 8 ft 0 in)" (IFCTEXT)
    PlatformSize = "0.91 m x 2.44 m (3 ft 0 in x 8 ft 0 in)" (IFCTEXT)
    ProductPageLink = "https://www.boels.com/en-nl/hire/telescopic-boom-lift-43-m/p/18034" (IFCTEXT)
    Swing = "360 degree Continuous" (IFCTEXT)
    TiltAlarmIndicatorLight = "5 Degree" (IFCTEXT)
    TurningRadiusInsideAxlesExtended = "2.44 m (8 ft 0 in)" (IFCTEXT)
    TurningRadiusInsideAxlesRetracted = "4.39 m(14 ft 5 in)" (IFCTEXT)
    TurningRadiusOutsideAxlesExtended = "5.89 m (19 ft 4 in)" (IFCTEXT)
    TurningRadiusOutsideAxlesRetracted = "6.86 m (22 ft 6 in)" (IFCTEXT)
    Tyres = "445/50D710 Foam Filled" (IFCTEXT)
    UniqueModelReferenceFAPL = "1001261213" (IFCTEXT)
  Model Properties | properties | on 1 type object
    BIMObjectName = "BoelsRental_18034_TelescopicBoomLift_JLG_1350SJP" (IFCTEXT)
    NBSDescription = "Lift platforms" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSObjectName = "Boels Rental - Lift platforms" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "n/a" (IFCTEXT)
    _Author = "Boels (JLG)" (IFCTEXT)
    _AuthorizedBy = "bimstore" (IFCTEXT)
    _BSBibleVersion = 17 (IFCINTEGER)
    _BimSpecGuid = 0 (IFCINTEGER)
    _CreatedBy = "https://www.boels.com/" (IFCTEXT)
    _CurrentRevision = 1 (IFCINTEGER)
    _DistributedBy = "https://www.boels.com/" (IFCTEXT)
    _ObjectUserGuide = "https://www.boels.com/" (IFCTEXT)