IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Time stamp: "2023-01-30T13:39:18"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190808_0900(x64) - Exporter 19.2.20.24 - Default UI"
Application: "Autodesk Revit 2019 (ENU)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENU)"

People and organizations
  Person "ryan.lashley24DJN" of Organization (no name given)
  Owner history of Person "ryan.lashley24DJN" of Organization (no name given) | application "Autodesk Revit 2019 (ENU)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENU)" | change NOCHANGE | created 1675085943 (2023-01-30T13:39:03Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCTRANSPORTELEMENT | type IFCTRANSPORTELEMENTTYPE "Height=-0.75m(-2'-6")_Reach=6.30m(20'-8")_(Platform Rotation 90°)" | object type "Height=-0.75m(-2'-6")_Reach=6.30m(20'-8")_(Platform Rotation 90°)" | ELEVATOR | names: "BoelsRental_18128_TelescopicBoomLift_JLG_660SJC:Height=-0.75m(-2'-6")_Reach=6.30m(20'-8")_(Platform Rotation 90°):26160" | material: materials ("BoelsRental_Plastic_Red", "BoelsRental_Plastic_Green", "BoelsRental_LightBlack", "BoelsRental_Plastic_Yellow", "BoelsRental_Grey", "JLG_Metal Paint_White", "JLG_Metal Paint_Black", "BoelsRental_PrimaryMaterial", "JLG_Paint_Orange", "BoelsRental_LogoWhite", "BoelsRental_LogoBlack", "BoelsRental_Tire") | property sets: Pset_ManufacturerTypeInformation, Constraints, Construction, Dimensions, Other, Phasing

Types
  IFCTRANSPORTELEMENTTYPE "Height=-0.75m(-2'-6")_Reach=6.30m(20'-8")_(Platform Rotation 90°)" | 1 occurrence | material: materials ("BoelsRental_Plastic_Red", "BoelsRental_Plastic_Green", "BoelsRental_LightBlack", "BoelsRental_Plastic_Yellow", "BoelsRental_Grey", "JLG_Metal Paint_White", "JLG_Metal Paint_Black", "BoelsRental_PrimaryMaterial", "JLG_Paint_Orange", "BoelsRental_LogoWhite", "BoelsRental_LogoBlack", "BoelsRental_Tire") | property sets: Constraints, Data, Identity Data, Model Properties, Other

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCTRANSPORTELEMENT)
    Manufacturer = "Boels Rental (JLG)" (IFCLABEL)
    ModelReference = "Telescopic Boom Lift" (IFCLABEL)
    ProductionYear = "2023" (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCTRANSPORTELEMENT)
    Host = "None" (IFCTEXT)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    P2 = FALSE (IFCBOOLEAN)
    P4 = FALSE (IFCBOOLEAN)
    PR = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Sa1 = 180. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 type object
    A = 20.5 (IFCLENGTHMEASURE) [MILLI METRE]
    A2a = -9.71 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    A2a1 = 170.29 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    AEa = -9.71 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    AEa1 = 170.29 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    AHa = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    AHa1 = 180. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Aa = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Aa1 = 180. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    JHa = 9.71 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    JHa1 = 189.71 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Ja = -61. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Ja1 = 119. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    P250 = TRUE (IFCBOOLEAN)
    P340 = TRUE (IFCBOOLEAN)
    PH2a = 61. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    PH2a1 = 241. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reach = 1 (IFCINTEGER)
  Construction | properties | on 1 object (1 IFCTRANSPORTELEMENT)
    PlatformRotation = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    ReachDiagram = FALSE (IFCBOOLEAN)
    SwingAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    WorkingArea = FALSE (IFCBOOLEAN)
  Dimensions | properties | on 1 object (1 IFCTRANSPORTELEMENT)
    Area = 824.248618486369 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 6.83783695943613 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCTRANSPORTELEMENT)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "Please Record On Commissioning." (IFCTEXT)
    Category = "Site" (IFCLABEL)
    Family = "BoelsRental_18128_TelescopicBoomLift_JLG_660SJC: Height=-0.75m(-2'-6")_Reach=6.30m(20'-8")_(Platform Rotation 90°)" (IFCLABEL)
    Family and Type = "BoelsRental_18128_TelescopicBoomLift_JLG_660SJC: Height=-0.75m(-2'-6")_Reach=6.30m(20'-8")_(Platform Rotation 90°)" (IFCLABEL)
    InstallationDate = "Please Record On Commissioning." (IFCTEXT)
    SerialNumber = "Please Record On Commissioning." (IFCTEXT)
    Type = "BoelsRental_18128_TelescopicBoomLift_JLG_660SJC: Height=-0.75m(-2'-6")_Reach=6.30m(20'-8")_(Platform Rotation 90°)" (IFCLABEL)
    Type Id = "BoelsRental_18128_TelescopicBoomLift_JLG_660SJC: Height=-0.75m(-2'-6")_Reach=6.30m(20'-8")_(Platform Rotation 90°)" (IFCLABEL)
    WarrantyStartDate = "Please Record On Commissioning." (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Level 1" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level: Level 1" (IFCLABEL)
    Type Id = "Level: Level 1" (IFCLABEL)
  Other | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Movable" (IFCTEXT)
    Category = "Site" (IFCLABEL)
    ClassificationName = "Uniclass2015" (IFCTEXT)
    ClassificationValue = "TE_30_30_10_60" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    CreatedBy = "https://www.boels.com/" (IFCTEXT)
    CreatedOn = "2023-01-24T09:30:00" (IFCTEXT)
    DocumentationCertificates = "https://www.boels.com/" (IFCTEXT)
    DocumentationInstallationGuide = "https://www.boels.com/" (IFCTEXT)
    DocumentationLiterature = "https://www.boels.com/" (IFCTEXT)
    DocumentationMaintenance = "https://www.boels.com/" (IFCTEXT)
    DocumentationTechnical = "https://www.boels.com/" (IFCTEXT)
    DurationUnit = "Years" (IFCTEXT)
    ExpectedLife = 0 (IFCINTEGER)
    Family Name = "BoelsRental_18128_TelescopicBoomLift_JLG_660SJC" (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Finish = "n/a" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    ManufacturerName = "Boels Rental (JLG)" (IFCTEXT)
    Material = "n/a" (IFCTEXT)
    ModelNumber = "Telescopic Boom Lift - 660SJC" (IFCTEXT)
    ModelReference = "Telescopic Boom Lift" (IFCTEXT)
    ProductionYear = "2023" (IFCTEXT)
    ReferencedStandard = "n/a" (IFCTEXT)
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "n/a" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    TypeName = "Height=-0.75m(-2'-6")_Reach=6.30m(20'-8")_(Platform Rotation 90°)" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "0" (IFCTEXT)
    WarrantyDurationParts = "0" (IFCTEXT)
    WarrantyDurationUnit = "Years" (IFCTEXT)
    WarrantyGuarantorLabor = "https://www.boels.com/" (IFCTEXT)
    WarrantyGuarantorParts = "https://www.boels.com/" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCTRANSPORTELEMENT)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "E1030100" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Cost = 0. (IFCREAL)
    Description = "n/a" (IFCTEXT)
    Keynote = "X" (IFCTEXT)
    Manufacturer = "Boels Rental (JLG)" (IFCTEXT)
    Model = "Telescopic Boom Lift - 660SJC" (IFCTEXT)
    OmniClass Number = "23.40.00.00" (IFCTEXT)
    OmniClass Title = "Equipment and Furnishings" (IFCTEXT)
    Type Comments = "Height=-0.75m(-2'-6")_Reach=6.30m(20'-8")_(Platform Rotation 90°)" (IFCTEXT)
    Type Name = "Height=-0.75m(-2'-6")_Reach=6.30m(20'-8")_(Platform Rotation 90°)" (IFCTEXT)
    URL = "https://www.boels.com/" (IFCTEXT)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Data | properties | on 1 type object
    ArticulatingJib = "1.83 m (6 ft 0 in)articulating jib" (IFCTEXT)
    AuxiliaryPower = "12V" (IFCTEXT)
    BoelsProductName = "Telescopic boom lift 22m high capacity 4x4" (IFCTEXT)
    BoelsSubgroup = "18128" (IFCTEXT)
    DieselEngine = "Deutz TD 2.9L4, 50kW (67 hp)" (IFCTEXT)
    DriveSpeed4WD = "2.57kph (1.6mph)" (IFCTEXT)
    FuelTankCapacity = "117L (31 gal)" (IFCTEXT)
    Gradeability4WD = "55%" (IFCTEXT)
    HorizontalOutreachRestricted = "14.62m (47 ft 11.5 in)" (IFCTEXT)
    HorizontalOutreachUnrestricted = "17.39m (57 ft 0.6 in)" (IFCTEXT)
    HydraulicPlatformRotator = "180 degree powered platform rotator" (IFCTEXT)
    HydraulicTankCapacity = "129 L (34 gal)" (IFCTEXT)
    JibOverallLength = "1.83m ( 6 ft 0 in)" (IFCTEXT)
    JibRangeOfArticulation = "132° (+71° / - 61°)" (IFCTEXT)
    MachineWeightANSI = "13,308kg (29,339 lbs)" (IFCTEXT)
    MachineWeightCE = "13,308kg (29,339 lbs)" (IFCTEXT)
    MaxGroundBearingPressureANSI = "0.79 kg/cm2 (11.2 psi)" (IFCTEXT)
    MaxGroundBearingPressureCE = "0.79 kg/cm2 (11.2 psi)" (IFCTEXT)
    ModelName = "660SJC" (IFCTEXT)
    NumberOfPeople = 0 (IFCINTEGER)
    PlatformCapacityRestrictedANSI = "340kg (750 lbs)" (IFCTEXT)
    PlatformCapacityRestrictedCE = "340kg (750 lbs)" (IFCTEXT)
    PlatformCapacityUnrestrictedANSI = "250kg (550 lbs)" (IFCTEXT)
    PlatformCapacityUnrestrictedCE = "250kg (550 lbs)" (IFCTEXT)
    PlatformHeightRestricted = "19.99m (65 ft 7 in)" (IFCTEXT)
    PlatformHeightUnrestricted = "19.99m (65 ft 7 in)" (IFCTEXT)
    PlatformRotator = "180 Degrees" (IFCTEXT)
    PlatformSideEntry = "0.91 m x 2.44 m low mount platform" (IFCTEXT)
    PlatformSize = "0.91 m x 2.44 m (3 ft 0 in x 8 ft 0 in)" (IFCTEXT)
    ProductPageLink = "n/a" (IFCTEXT)
    Swing = "360 Degrees Continuous" (IFCTEXT)
    TiltAlarmIndicatorLight = "5 degree tilt alarm and indicator light" (IFCTEXT)
    UniqueModelReferenceFAPL = "1001188600" (IFCTEXT)
  Model Properties | properties | on 1 type object
    BIMObjectName = "BoelsRental_18128_TelescopicBoomLift_JLG_660SJC" (IFCTEXT)
    NBSDescription = "Lift platforms" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSObjectName = "Boels Rental - Lift platforms" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "n/a" (IFCTEXT)
    _Author = "Boels (JLG)" (IFCTEXT)
    _AuthorizedBy = "bimstore" (IFCTEXT)
    _BSBibleVersion = 17 (IFCINTEGER)
    _BimSpecGuid = 0 (IFCINTEGER)
    _CreatedBy = "https://www.boels.com/" (IFCTEXT)
    _CurrentRevision = 1 (IFCINTEGER)
    _DistributedBy = "https://www.boels.com/" (IFCTEXT)
    _ObjectUserGuide = "https://www.boels.com/" (IFCTEXT)